2023-9-15

to add side key functions assignment for these two keys, so these two keys now are programmable, to use these function, please kindly note that your programming software should be V1.08 released on 09.Sept, 2023

Programming software: UV99\_20230909\_V1.08

Firmware: UV99\_Eng\_Upadat\_20230915\_B91.21

VOX

Dual wait

scan

monitor

1750Hz tone

flashlight

power select

alarming

noise cancellation function

temporary monitor

FM radio

talk around

Frequency reverse

2023-5-9

1、after reset, channel name won't be removed completely

2、transmission will be error when you set TX DCS to it

3、channel name storage error

2023-4-21

1、solve the issue that while current channel is receiving a call and you change the channel (or frequency) by up and down buttons, click-clack sound is heard from speaker and you hear continuous background noise (hssshhhhhh) from sepeaker

2023-2-18

1、address the issue that there is a sound "click-clack" during scan

2023-1-13

1、to enable the access to VFO in CH mode by press #

2、to address the issue of wrong display if you turn off display name in menu 22

1、please press PTT to power on and LED will display Update......

2、open the updating software and set Baud rate as 57600 and choose the correct com port

open the firmware and press update

